ASA-5512# copy tftp: disk0:

Address or name of remote host []? 172.16.31.1

Source filename []? asa916-smp-k8.bin

Destination filename [asa916-smp-k8.bin]?

Accessing tftp://172.16.31.1/asa916-smp-k8.bin...!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

Writing file disk0:/asa916-smp-k8.bin...

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

38043648 bytes copied in 32.290 secs (1188864 bytes/sec)

ASA-5512# sh disk0  
--#--  --length--  -----date/time------  path

**191  38191104    Nov 21 2014 21:07:48  asa912-smp-k8.bin  
 192  17906032    Apr 08 2015 22:33:44  asdm-713.bin  
  193  26350916    Apr 09 2015 06:28:20  asdm-741.bin  
  194  38043648    May 10 2015 02:14:06  asa916-smp-k8.bin**4118732800 bytes total (3556712448 bytes free)

!--- Command to set "asa916-smp-k8.bin" as the boot image.

ASA-5512(config)# **boot system disk0:/asa916-smp-k8.bin**

!--- Command to set "asdm-741.bin" as the ASDM image.

ASA-5512(config)# **asdm image disk0:/asdm-741.bin**

ASA-5512# **write memory**

ASA-5512# **reload**

<http://www.cisco.com/c/en/us/support/docs/security/asa-5500-x-series-next-generation-firewalls/200142-ASA-9-x-Upgrade-a-Software-Image-using.html>

Compatibilidade de imagens

http://www.cisco.com/c/en/us/td/docs/security/asa/compatibility/asamatrx.html